## DTC Troubleshooting: 45, 46, 47, 48

DTC 45, 46, 47, 48: | VSA Solenoid

1. | Clear the DTCs using the HDS.

2. | Turn the ignition switch ON (II).

3. | Check the DTCs using the HDS. Does the ABS indicator come on, and are DTCs 45, 46, 47, 48 indicated? YES - Check for loose or poor connections in the VSA control unit 46P connector. If connections are good, replace the VSA modulator-control unit.n NO - The system is OK at this time.n