## DTC Troubleshooting: 24-1

DTC 24-1: | Open or Increased Resistance in Right Side Seat Belt Outer Lap Tensioner

Special Tools Required
SRS inflator simulator ( 07SAZ-TB4011A)

SRS simulator lead E ( 07XAZ-S1A0200)

1. | Erase the DTC memory.

2. | Turn the ignition switch ON (II), and check that the SRS indicator comes on for about 6 seconds and then goes off. Does the SRS indicator stay on? YES - Go to 3. NO - Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures.n

3. | Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes.

4. | Disconnect the TBR1o connector from the TBR1i connector (A).

5. | Connect the special tool (2 W connector) to the TBR1i connector.

6. | Reconnect the battery negative cable.

7. | Erase the DTC memory.

8. | Read the DTC. Is DTC 24-1 indicated? YES - Go to 9. NO - Open or increased resistance in the right side seat belt outer lap tensioner; replace the right side seat belt.n

9. | Disconnect the battery negative cable, and wait for 3 minutes.

10. | Disconnect the both seat belt tensioner 4P connectors from the floor wire harness 4P connectors.

11. | Disconnect the TBL1o connector (A) from the TBL1i connector (B).

12. | Disconnect the U2o connector (A) from the SRS unit.

13. | Check resistance between the No. 9 terminal and the No. 10 terminal of U2o connector (28P). There should be 2.0-3.0 W. Is the resistance as specified? YES - Faulty SRS unit or poor contact at U2o connector (28P) and the SRS unit, check the connection between the U2o connector (28P) and the SRS unit. If the connection is OK, replace the SRS unit.n NO - Open or increased resistance in the floor wire harness; replace the floor wire harness.n