## Sunroof Limit Switch Test

## OPEN/CLOSE, TILT/CLOSE SWITCH:

1. | Remove the headliner

2. | Disconnect the 4P connector from the sunroof limit switch.

3. | Check for continuity between the terminals in each switch position according to the table. NOTE: Turn the motor by hand with the wrench.

## OPEN SWITCH (KK, KU and KT models):

1. | Remove the headliner.

2. | Disconnect the 4P connector from the sunroof limit switch.

3. | Check for continuity between the terminals in each switch position according to the table. NOTE: Turn the motor by hand with the wrench.