## Camshaft Removal

1. | Remove the air cleaner housing.

2. | Remove the camshaft sprocket.

3. | Remove the rocker arm assembly.

4. | Remove the air cleaner housing bracket, ground cable and harness holder mounting bolt, then remove the harness holder from the bracket.

5. | Disconnect the camshaft position (CMP) (top dead center (TDC)) sensor, connector, then remove the CMP (TDC) sensor, refer to the 2002 Jazz/Fit Shop Manual.

6. | Remove the camshaft thrust cover (A), then pull out the camshaft (B).