## 7-speed Mode Main Switch/Steering Shift Switch Test

SRS components are located in this area. Review the following articles in the SRS section before performing repairs or service;

- Component Locations.
- Precautions and Procedures.

1. | Remove the steering column covers upper and lower.

2. | Remove the driver's airbag from the steering wheel.

3. | Disconnect the main switch (7SPEED MODE)/steering shift switch connector (A).

4. | Check the main switch (7SPEED MODE) for continuity between connector terminals No. 1 and No. 2. There should be toggled continuity and no continuity between terminals every time the main switch (7SPEED MODE) (B) pushes.

5. | Check the steering shift switch plus (+) for continuity between connector terminals No. 4 and No. 2. There should be continuity while pressing both plus (+) of the steering shift switches, and no continuity when the plus (+) switch released.

6. | Check the steering shift switch minus (-) for continuity between connector terminals No. 3 and No. 2. There should be continuity while pressing both minus (-) of the steering shift switches, and no continuity when the minus (-) switch released.

7. | If either test is faulty, replace the main switch ( 7SPEED MODE)/steering shift switch. If the switch is OK, repair the wire harnesses between the cable reel and the PCM.