## A/T Shift Lock Solenoid Test

1. | Remove the center console.

2. | Remove the shift lock solenoid/park pin switch connector from the shift lever bracket base, then disconnect the connector.

3. | Connect the battery positive terminal to shift lock solenoid connector terminal No. 1, and connect the battery negative terminal to the terminal No. 3. NOTE: Do not connect the battery positive terminal to the terminal No. 3 or you will damage the diode inside the shift lock solenoid.

4. | Check that the shift lever can be moved from the [P] position. Release the battery terminals from the shift lock solenoid connector. Move the shift lever back to the [P] position, and make sure it locks.

5. | Check that the shift lock releases when the shift lock release is pushed, and check that it locks when the shift lock release is released.

6. | If the shift lock solenoid works improperly, replace it.