## M/T Countershaft Disassembly

1. | Securely clamp the countershaft assembly in a bench vise with wood blocks.

2. | Use a chisel (A) to raise the locknut tab (B) from the groove in the countershaft.

3. | Remove the locknut (left-hand threads) (A) and the spring washer (B).

4. | Support 5th gear (A) on steel blocks (B), then use a press (C) and an attachment (D) to press the countershaft (E) out of the ball bearing (F).

5. | Support 4th gear (A) on steel blocks (B), then use a press (C) and an attachment (D) to press the countershaft (E) out of the 4th gear.

6. | Support 3rd gear (A) on steel blocks (B), then use a press (C) and an attachment (D) to press the countershaft (E) out of the 3rd gear.