Steering
Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Steering wheel | Rotational play measured at outside edge with engine running |  | 0-10 mm (0-0.39 in.)
Starting load measured at outside edge with engine running |  | 29 N (3.0 kgf, 6.6 lbs)
Gearbox | Angle of rack guide screw loosened from locked position |  | 12° Max.

Suspension
Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Wheel alignment | Camber | Front | 0°00¢±1°
Rear | -1°00¢±1¢
Caster | Front | 2°10¢±1°
Total Toe | Front | 0±3 mm (0±0.12 in.)
Rear | IN 2±2 mm (2± 0.08 in.)
Front wheel turning angle equipped with 175/65 R14 82T tyres | Inside wheel | 41°00¢
Outside wheel | 36°(Reference)
Front wheel turning angle equipped with 185/55 R15 82V tyres | Inside wheel | 38°00¢±2°
Outside wheel | 34°(Reference)
Wheel | Steel wheel runout | Axial | 0-1.0 mm (0-0.04 in.) | 2.0 mm (0.08 in.)
Radial | 0-1.0 mm (0-0.04 in.) | 1.5 mm (0.06 in.)
Aluminum wheel runout | Axial | 0-0.7 mm (0-0.03 in.) | 2.0 mm (0.08 in.)
Radial | 0-0.7 mm (0-0.03 in.) | 1.5 mm (0.06 in.)
Wheel bearing | End play | Front | 0-0.05 mm (0-0.002 in.)
Rear | 0-0.05 mm (0-0.002 in.)

Brakes
Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Parking brake lever | Distance travelled when lever pulled with 196 N (20 kgf, 44 lbs) of force |  | 7-10 clicks
Brake pedal | Pedal height (Carpet removed) | M/T | 141 mm (5 9/16 in.)
CVT | 145 mm (5 11/16 in.)
Free play |  | 1-5 mm (0.04-0.2 in.)
Master cylinder | Piston-to-pushrod clearance |  | 0-0.4 mm (0-0.02 in.)
Front brakes (disc brake) | Disc thickness |  | 21.0 mm (0.83 in.) | 19.0 mm (0.75 in.)
Disc runout |  | ——— | 0.10 mm (0.004 in.)
Disc parallelism |  | ——— | 0.015 mm (0.0006 in.)
Pad thickness |  | 9.0 mm (0.35 in.) | 1.6 mm (0.06 in.)
Rear brake s | Brake drum I.D. |  | 180 mm (7.09 in.) | 181 mm (7.13 in.)
Brake shoe lining thickness |  | 4.3 mm (0.17 in.) | 1.0 mm (0.039 in.)
Brake booster | Master cylinder fluid pressure at 0 kPa (0 mmHg, 0 in. Hg) of vacuum with pressing brake pedal | Pressed with 98 N (10 kgf, 22 lbs) | 0 kPa (0 kgf/cm2, 0 psi)
Pressed with 290 N (30 kgf, 66 lbs) | 1,600 kPa (16 kgf/cm2, 230 psi)
Master cylinder fluid pressure at 66.7 kPa (500 mmHg, 19.7 in. Hg) of vacuum with pressing brake pedal | Pressed with 98 N (10 kgf, 22 lbs) | 3,400 kPa (34 kgf/cm2, 480 psi)
Pressed with 290 N (30 kgf, 66 lbs) | 9,800 kPa (98 kgf/cm2, 1,400 psi)
Brake booster | Master cylinder fluid pressure at 0 kPa (0 mmHg, 0 in. Hg) of vacuum with pressing brake pedal | Pressed with 98 N (10 kgf, 22 lbs) | 0 kPa (0 kgf/cm2, 0 psi)
Pressed with 290 N (30 kgf, 66 lbs) | 1,600 kPa (16 kgf/cm2, 230 psi)
Master cylinder fluid pressure at 66.7 kPa (500 mmHg, 19.7 in. Hg) of vacuum with pressing brake pedal | Pressed with 98 N (10 kgf, 22 lbs) | 3,700 kPa (37 kgf/cm2, 530 psi)
Pressed with 290 N (30 kgf, 66 lbs) | 9,800 kPa (98 kgf/cm2, 1,400 psi)

Air Conditioning
Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Refrigerant | Type |  | HFC-134 a (R-134 a)
Capacity of system |  | 400-450 g (14.1-15.9 oz)
Refrigerant oil | Type |  | KEIHIN: SP-10 (P/N 38897-P13-A01AH, 38898-P13-003, 38899-P13-A01)
Capacity of components | Condenser | 25 mL (5/6 fl oz, 0.9 lmp oz)
Evaporator | 35 mL (1 1/6 fl oz, 1.2 lmp oz)
Each line and hose | 10 mL (1/3 fl oz, 0.4 lmp oz)
Compressor | 85-105 mL (2 1/6-3 1/2 fl oz, 3.0-3.7 lmp oz)
Compressor | Starter coil resistance | at 68°F (20°C) | 3.05-3.35 W
Pulley-to-pressure plate clearance |  | 0.35-0.65 mm (0.014-0.026 in.)
Alternator- compressor belt | Deflection with 98 N (10 kgf, 22 lbs) applied mid-way between pulleys | Used belt | 7.5-10.5 mm (0.30-0.413 in.)
New belt | 4.5-6.0 mm (0.18-0.24 in.)
Tension (measured with belt tension gauge) | Used belt | 440-590 N (45-60 kgf, 99-130 lbs)
New belt | 980-1,130 N (100-115 kgf, 220-254 lbs)