## Glass Adjustment

NOTE: Check the weatherstrips and glass run channel for damage or deterioration, and replace them if necessary.

1. | Place the vehicle on a firm, level surface.

2. | Remove these items: Door panel, front door, rear door Plastic cover, front door, rear door

3. | Carefully move the glass (A) until you can see the glass mounting bolts (B), then loosen them. Front: Rear:

4. | Push the glass (A) against the channel (C), then tighten the glass mounting bolts.

5. | Check that the glass moves smoothly.

6. | Raise the glass fully, and check for gaps. Also check that the glass (A) contacts the glass run channel (B) evenly.

7. | Check for water leaks. Run water over the roof and on the sealing area as shown, and note these items: Use a 12 mm (0.47 in.) diameter hose (A). Adjust the rate of water flow as shown (B). Do not use a nozzle. Hold the hose about 300 mm (12 in.) away from the door (C).

8. | Attach the plastic cover, and install the door panel, front door, rear door.