## HID Unit Replacement

1. | Turn the combination light switch OFF.

2. | Disconnect the battery negative cable, then disconnect the positive cable.

3. | Remove the headlight assembly.

4. | Remove the bulb socket from the HID bulb.

5. | Remove the three mounting screws from the headlight housing (A).

6. | Disconnect the connector (B) and remove the HID unit.

7. | Install in the reverse order of removal.