## Radiator Test

1. | Wait until the engine is cool, then carefully remove the radiator cap and fill the radiator with engine coolant to the top of the filler neck.

2. | Attach the pressure tester (A) (commercially available) to the radiator. Use a small adapter H-901122-09 (B) (commercially available) to attach the pressure tester.

3. | Apply a pressure of 93-123 kPa (0.95-1.25 kgf/cm2, 14-18 psi).

4. | Inspect for engine coolant leaks and a drop in pressure.

5. | Remove the tester, and reinstall the radiator cap.

6. | Check for engine oil in the coolant and/or coolant in the engine oil.