## A/C Compressor Clutch Check

1. | Check the armature plate for discoloration, peeling, or other damage. If there is damage, replace the clutch set.

2. | Check the rotor pulley bearing play and drag by rotating the rotor pulley by hand. Replace the clutch set with a new one if it is noisy or has excessive play/drag.

3. | Measure the clearance between the rotor pulley (A) and the armature plate (B) all the way around. If the clearance is not within specified limits, remove the armature plate and add or remove shims as needed to increase or decrease clearance.
Clearance: | 0.5±0.15 mm (0.020±0.006 in.)
NOTE: The shims are available in four thicknesses: 0.1 mm, 0.2 mm, 0.4 mm, and 0.5 mm.

4. | Release the field coil connector from the holder, then disconnect it. Check the thermal protector for continuity. If there is no continuity, replace the thermal protector. NOTE: The thermal protector will have no continuity above 122 to 132°C (252 to 270°F). When the temperature drops below 116 to 104°C (241 to 219°F), the thermal protector will have continuity.

5. | Check resistance of the field coil. If resistance is not within specifications, replace the field coil.
Field Coil Resistance: | 3.05-3.35 ohms at 20°C (68°F)