## Transmission Range Switch Test

1. | Remove the air cleaner housing and intake air duct.

2. | Disconnect the transmission range switch connector.
Connector Terminal Specifications
Connector Terminal | Signal
--- | ---
1 | -
2 | [N]
3 | [S]
4 | ST
5 | -
6 | [P]
7 | [R]
8 | [D]
9 | [L]
10 | GND

3. | Check for continuity between terminals at the connector. There should be continuity between terminals in the following table for each switch position. Transmission Range Switch Continuity check

4. | If there is no continuity between any terminals, adjust the transmission range switch installations. If the transmission range switch installation is OK, replace the transmission range switch.