## Power Assist Check

## Power Steering:

1. | Start the engine, let it idle, and turn the steering wheel from lock-to-lock several times to warm up.

2. | Attach a commercially available spring scale to the steering wheel. With the engine idling and the vehicle on a clean, dry floor, pull the scale as shown and read it as soon as the tires begin to turn.

3. | If the scale reads no more than 29N (3.0 kgf, 6.6 lbf). If it reads more, check for steering linkage.