## Rack Guide Adjustment

Special Tools Required
Locknut wrench, 40 mm ( 07MAA-SL00100)

1. | Set the wheels in the straight ahead position.

2. | Loosen the rack guide screw locknut (A) with the special tool, then remove the rack guide screw (B). LHD: RHD:

3. | Remove the old sealant from rack guide screw, and apply new sealant all around the threads (A).

4. | Loosely install the rack guide screw (A) on the steering gearbox.

5. | Tighten the rack guide screw to 25 N·m (2.5 kgf·m, 18 lbf·ft), then loosen it.

6. | Retighten the rack guide screw to 3.9 N·m (0.4 kgf·m, 2.9 lbf·ft) then back it off to specified angle.
Specified Return Angle: | 12° Max.

7. | Tighten the locknut (B) while holding the rack guide screw (A).

8. | Check for unusual steering effort through the complete turning travel.

9. | Check the steering wheel rotational play and the power assist.