## Audio Unit Removal/Installation

1. | Remove the center panel.

2. | Disconnect the 20P connector and antenna lead from the audio unit.

3. | Disconnect the connectors from the heater control panel.

4. | Disconnect the connector from the rear window defogger switch.

5. | Remove the seven mounting screws, then remove the audio unit (A).

6. | Remove the four mounting screws from the LCD unit (A), then remove the cover (B).

7. | Remove the two knobs (A).

8. | Remove the sixteen mounting screw from the printed circuit board (B), then remove the printed circuit board and LCD unit.

9. | Install the reverse order of removal. NOTE: Do not remove the connection of the printed circuit board and the LCD unit.