## Rocker Arm Assembly Removal

1. | Remove the cylinder head cover.

2. | Loosen the rocker arm adjusting screws (A).

3. | Unscrew the rocker shaft mounting bolts two turns at a time, in sequence below.

4. | Remove the rocker shaft mounting bolts, then remove the rocker arm assembly (A). NOTE: When disassembling the rocker arms, remove the dowel pin (B), then remove the rocker arm from cam chain side on the rocker shaft.