## HID Cord Complete Replacement

1. | Remove the headlight.

2. | Remove the HID bulb from the headlight.

3. | Disconnect the 2P connector (A) from the high/low beam switching solenoid (B).

4. | Turn the connector (C) 45° counterclockwise to remove it from the headlight housing (D).

5. | Slide the diode (E) up and remove the cord complete (F).

6. | Install in the reverse order of removal.

7. | After replacement, adjust the headlight.