## Taillight Replacement

1. | Remove the rear bumper.

2. | Open the tailgate and remove the maintenance lid.

3. | Disconnect the connectors (A) from the taillight (B).
Brake/Taillight: | 21/5 W
Turn Signal Light: | 21 W
Back-Up Light: | 21 W
Rear Fog Light: | 21 W (KG,KR and KE models)

4. | Remove the mounting nuts and the screw, then remove the taillight.

5. | When installing the taillight, check for the gasket; if it is distorted or stays compressed, replace it.

6. | After installing the taillight, run water over the taillight to make sure they do not leak.