## Power Mirror Replacement

1. | Raise the door glass fully.

2. | Remove these items: Door panel Plastic cover, as necessary

3. | Disconnect the connector (A).

4. | Detach the harness clip (B).

5. | Remove the maintenance cap (A), and remove the nuts. While holding the mirror, detach the clip (B), then remove the mirror (C). Take care not to scratch the door.

6. | Install the mirror in the reverse order of removal, and make sure the connector is plugged in properly.