## Headlight Adjuster Switch Test

1. | Remove the power mirror switch.

2. | Carefully push out the headlight adjuster switch (A) from behind the dashboad.

3. | Disconnect the 5P connector (B) from the switch.

4. | Measure resistance between the No. 1 and No. 3 terminals and No. 2 and No. 3 terminals at positions 0, 1, 2, and 3 by moving the switch knob.
Between the No. 1 and No. 3 terminals:
About 4.7 kW
Between the No. 2 and No. 3 terminals:
Knob position | 0 | 1 | 2 | 3
Resistance [About (kW)] | 0.7 | 1.4 | 1.6 | 2.0