## M/T Countershaft Bearing Replacement

Special Tools Required
Adjustable bearing puller, 25-40 mm ( 07JAC-PH80100)

Bearing remover shaft ( 07JAC-PH80200)
Slide hammer ( 07741-0010201)
Driver ( 07749-0010000)
Attachment, 52 x 55 mm ( 07746-0010400)

1. | Remove the needle bearing (A) using the special tool, then remove the oil guide plate C.

2. | Position the oil guide plate C and new needle bearing (A) in the bore of the clutch housing (B).

3. | Install the needle bearing using the special tools.