## Side Impact Sensor Replacement

## Removal

NOTE:

- Removal of the side impact sensor must be performed according to the precautions/procedures described before.
- Before disconnecting the side impact sensor 2P connector(s), disconnect the side airbag 2P connector(s).
- Do not turn the ignition switch ON (II) and do not connect the battery cable while replacing the side impact sensor.

1. | Disconnect the negative battery cable, and wait at least 3 minutes before beginning work.

2. | Remove the seat assembly.

3. | Remove the rear side trim panel.

4. | Disconnect the floor wire harness 2P connector from the side impact sensor.

5. | Remove the Torx bolt (A) using a Torx T30 bit, then remove the side impact sensor (B).

## Installation

NOTE:

- Be sure to install the harness wires so that they are not pinched or interfering with other parts.
- Do not turn the ignition switch ON (II) and do not connect the battery cable while replacing the side impact sensor.

1. | Install the new side impact sensor with a new Torx bolt (A) then connect the floor wire harness 2P connector (B) to the side impact sensor (C).

2. | Reconnect the negative battery cable.

3. | After installing the side impact sensor, confirm proper system operation: Turn the ignition switch ON (II): the SRS indicator should come on for about 6 seconds and then go off.