## Crankshaft Pulley Removal and Installation

Special Tools Required
Holder handle ( 07JAB-0010200)

Pulley holder attachment, HEX 50 mm ( 07JAB-0010400)
Socket wrench, 19 mm ( 07JAA-0010200)

## Removal

1. | Remove the front tires/wheels.

2. | Remove the splash shield.

3. | Hold the pulley with handle (A) and holder attachment (B).

4. | Remove the bolt with a 19 mm socket (C) and breaker bar.

## Installation

1. | Clean the crankshaft pulley (A), crankshaft (B), bolt (C), and washer (D). Lubricate as shown below.

2. | Install the crankshaft pulley, and hold the pulley with handle (A) and holder attachment (B).

3. | Tighten the bolt to 54 N·m (5.5 kgf·m, 40 lbf·ft) with a torque wrench and 19 mm socket (C). Do not use an impact wrench. If you are using a new pulley bolt or new crankshaft, tighten the bolt to 177 N·m (18.0 kgf·m, 130 lbf·ft) with a torque wrench and 19 mm socket, loosen the bolt and tighten it 54 N·m (5.5 kgf·m, 40 lbf·ft).

4. | Tighten the pulley bolt an additional 90°.

5. | Install the splash shield.

6. | Install front tires/wheels.