## Steering Lock Replacement

1. | Remove the steering column.

2. | Center punch each of the two shear bolts, and drill their heads off with a 5 mm (3/16 in.) drill bit. Be careful not to damage the switch body when removing the shear bolts.

3. | Remove the shear bolts from the switch body.

4. | Install the switch body without the key inserted.

5. | Loosely tighten the new shear bolts.

6. | Insert the ignition key, and check for proper operation of the steering wheel lock and that the ignition key turns freely.

7. | Tighten the shear bolts (A) until the hex heads (B) twist off.