## Alternator Replacement

1. | Disconnect the battery negative cable from the battery.

2. | Remove the intake manifold.

3. | Disconnect the alternator connector (A), WHT wire (B) and harness clamp (C) from the alternator.

4. | Remove the drive belt.

5. | Remove the lock bolt (A) and mounting bolt (B), then remove the alternator.

6. | Install the alternator in the reverse order of removal.

7. | Adjust the drive belt tension.

8. | Perform the ETCS learn procedure (with ETCS).