## Combination Light Switch Test/Replacement

1. | Remove the steering column covers.

2. | Disconnect the 16P connector (A) from the combination light switch (B). LHD type and KE model: RHD type except KE model:

3. | Remove the two screws, then slide out the combination light switch.

4. | Inspect the connector terminals to be sure they are all making good contact. If the terminals are bent, loose or corroded, repair them as necessary, and recheck the system. If the terminals look OK, check for continuity between the terminals in each switch position according to the tables.

5. | If there is no continuity, replace the switch.