## Manual Valve Body Disassembly, Inspection, and Reassembly

1. | Remove the spring seat (A), valve spring (B), and reverse inhibitor valve (C) from the manual valve body (D).
Reverse Inhibitor Valve Spring Specifications (Standard) Wire diameter: 1.1 mm (0.043 in.) Outside diameter: 7.0 mm (0.276 in.) Free length: 46.8 mm (1.843 in.) Number of coil: 21.4

2. | Remove the manual valve (E).

3. | Check the all part wear and damage.

4. | Clean all parts thoroughly in solvent or carburator cleaner, and dry with compressed air. Blow out all passages.

5. | Coat all parts with ATF during assembling.