## Sunroof Glass Height Adjustment

The roof panel (A) should be even with the glass weatherstrip (B), to within 2+0.5/-1 mm (0.08+0.02/-0.04 in.) all the way around. If not, make the following adjustment:

1. | Remove the bracket cover from each side.

2. | Loosen the nuts (A), and install the shims (B) between the glass frame (C) and glass bracket (D) on each side.
Shim thickness: | Front and rear max. 2 mm (0.08 in.)

3. | If necessary, repeat on the opposite side.