## DTC Troubleshooting: 65

DTC 65: | VSA Pressure Sensor (Hardwear)

1. | Clear the DTCs using the HDS.

2. | Turn the ignition switch OFF, then turn it ON (II).

3. | Verify the DTC. Is DTC 62 indicated? YES - Check for loose connection terminals in the VSA control unit 46P connector and repair If necessary. If terminals are OK, replace the VSA modulator-control unit.n NO - The system is OK at this time.n