## Tailgate Handle Replacement

NOTE: Put on gloves to protect your hands.

1. | Remove the rear license trim.

2. | Disconnect the tailgate opener cable (A) from the tailgate handle (B), and remove the nuts.

3. | From outside of the tailgate, pull out the tailgate handle, then remove it.

4. | Install the handle in the reverse order of removal, and note these items: Make sure the tailgate opener cable is connected securely. Make sure the tailgate opens properly.