## 7-speed Mode Steering Shift + (Plus) Switch Test

## For KB, KE, KG, and KQ (L15A1 engine) Models (6-position CVT+7Speed Mode)

SRS components are located in this area. Review the following articles in the SRS before performing repairs or service;

- Component Locations.
- Precautions and Procedures.

1. | Remove the steering wheel.

2. | Check the steering shift + (plus) switch for continuity between cable reel subharness 13P connector terminals No. 6 and No. 9. There should be continuity while pressing the steering shift + (plus) switch, and no continuity when the switch is released.

3. | Steering shift + (plus) switch test has finished if the test result is OK. If the switch works incorrectly at the 13P connector, test the switch at the switch connector.

4. | Remove steering shift + (plus) switch connector from its clamp, and disconnect the connector.

5. | Check the steering shift + (plus) switch for continuity between the switch connector terminals while pressing the steering shift + (plus) switch and when the switch is released. There should be continuity while pressing the steering shift + (plus) switch, and no continuity when the switch is released.

6. | Replace the steering shift + (plus) switch if the switch works incorrectly.

7. | Replace the cable reel subharness if the switch is OK.