## DTC Troubleshooting: 52

DTC 52: | Motor Stuck OFF

1. | Check the No. 4 (40A) fuse in the under-hood fuse/relay box, and reinstall the fuse if it is OK. Is the fuse OK? YES - Go to 2. NO - Replace the fuse, and recheck.n

2. | Disconnect the ABS control unit 25P connector.

3. | Measure the voltage between the ABS control unit 25P connector terminal No. 25 and body ground. Is there battery voltage? YES - Check for loose terminals in the ABS control unit 25P connector. If necessary, substitute a known-good ABS modulator-control unit, and recheck.n NO - Repair open in the wire between the No. 4 (40A) fuse and the ABS control unit.n