## Rear Hub Bearing Unit Replacement - Rear Drum Brake

### Exploded View

1. | Raise the rear of the vehicle, and make sure it is securely supported. Remove the rear wheels.

2. | Remove the hub cap (A), raise the stake (B), and remove the spindle nut (C).

3. | Release the parking brake. Screw two 8 x 1.25 mm bolts into the drum to push it away from the hub. Turn each bolt two turns at a time to prevent cocking the drum excessively. Remove the brake drum (A).

4. | Remove the hub bearing unit (A) from the spindle.

5. | Install the hub bearing unit in the reverse order of removal, and note these items: Tighten all mounting hardware to the specified torque values. Before installing the brake drum, clean the mating surface of the hub and the inside of the brake drum. Use a new spindle nut on reassembly. After tightening the spindle nut, use a drift to stake the spindle nut shoulder against the spindle. Use a new hub cap on reassembly. Before installing the wheel, clean the mating surface of the brake drum and the inside of the wheel.