## Fuse to Component Index

Under-hood fuse/relay box
Fuse Number | Amps | Wire Color | Component(s) or Circuit(s) Protected
--- | --- | --- | ---
1 | 80 A | ——— | Battery, Power distribution
2 | 40 A | WHT/BLU | EPS control unit
3 | 50 A | WHT | Ignition switch (BAT)
4 | 30 A | WHT/RED | VSA modulator-control unit
5 | 40 A | WHT/BLU | Blower motor
6 | 40 A | WHT | No. 2, 3, 4, 13 and 14 fuses (in the under-dash fuse/relay box)
7 | 30 A | BLU/RED | No. 18, 19 and 21 fuses (in the under-dash fuse/relay box), Sunroof motor
8 | 15 A | WHT/RED | Audio unit, Ceiling light, Data link connector, Gauge assembly, Immobilizer control unit-receiver, Immobilizer code unit, Keyless receiver unit, Navigation unit, Spotlights, Tailgate light
9 | 10 A | RED/BLK | Dash lights, Front parking lights, Gauge lights, License plate lights, Taillights
10 | 30 A | BLU/BLK | Radiator fan motor
11 | 30 A | BLU/YEL | A/C compressor clutch relay
BLU/RED | Condenser fan motor
12 | 20 A | RED | Right headlight
RED/WHT | Right headlight (HID unit, switching solenoid)
13 | 20 A | RED/YEL | Left headlight, High beam indicator
BLU/RED | Left headlight (HID unit, switching solenoid), High beam indicator
14 | 10 A | WHT/BLK | Turn signal/hazard flasher control circuit (Has built in gauge assembly)
15 | 30 A | WHT/GRN | VSA modulator-control unit
16 | 15 A | WHT/GRN | Brake lights, ECM, Shift lock control circuit (Has built in gauge assembly), VSA modulator-control unit
BLU/RED | Horn
Fuse/relay box socket | Horn relay

Under-dash Fuse/Relay Box
Fuse Number | Amps | Wire Color | Component(s) or Circuit(s) Protected
--- | --- | --- | ---
1 | 10 A | YEL | Back-up light (M/T)
2 | 15 A | BLK/RED | Ignition coil (rear)
3 | 7.5 A | YEL | Alternator, EPS control unit, ELD unit, EVAP canister purge valve, Gauge assembly, Headlight adjuster, Headlight adjuster switch, IMOES unit, Keyless receiver unit, Primary HO2S, Secondary HO2S, Vehicle speed sensor (M/T)
4 | 10 A | YEL/BLK | Turn signal/hazard flasher circuit (built into gauge assembly)
5 | 7.5 A | BLK/RED | ECM (with throttle actuator control)
6 | 20 A | GRN/BLK | Intermittent wiper control unit (built into wiper/washer switch), Rear washer motor, Windshield wiper motor, Windshield washer motor
7 | ——— | ——— | Not used
8 | ——— | ——— | Not used
9 | 20 A | BLK/ORN | Climate control unit (via rear window defogger relay), Rear window defogger (via rear window defogger relay)
10 | 7.5 A | BLK/YEL | A/C compressor clutch relay, A/C switch, Blower motor relay, Condenser fan relay, Climate control unit, Power mirror actuator, Power mirror defogger relay, Radiator fan relay
Fuse/relay box socket | Optional connector
11 | 15 A | BLK/YEL | ECM, Fuel pump, Inertia switch, Immobilizer control unit-receiver, SRS unit (VA)
12 | 10 A | GRN | Power window control unit (built into power window master switch), Rear window wiper motor
Fuse/relay box socket | Power window relay
13 | 10 A | PNK | SRS unit (VB)
14 | 15 A | WHT/BLK | CKP sensor, TDC sensor, ECM, Injectors, IAC valve, PGM-FI main relay1, PGM-FI main relay2
15 | 20 A | YEL/RED | Left rear power window motor (via power window switch)
16 | 20 A | YEL/BLU | Right power window motor (via power window switch)
17 | 20 A | GRN/BLK | Front passenger's power window motor (via power window switch)
18 | 10 A | WHT/GRN | Rear fog light control unit (with front fog light)
19 | 20 A | BLU/RED | Power mirror defogger (via power mirror defogger relay), Sunroof motor
20 | ——— | ——— | Not used
21 | 20 A | BLU/BLK | Front fog light
22 | ——— | ——— | Not used
23 | ——— | ——— | Not used
24 | 15 A | BLK/WHT | Ignition coil (front)
25 | 7.5 A | YEL | VSA modulator-control unit (IG1)
26 | 7.5 A | YEL/RED | Audio unit (without navigation), AVN unit (with navigation), Navigation unit
Fuse/relay box socket | Optional connector
27 | 15 A | YEL/GRN | Cigarette lighter
28 | 20 A | WHT | Door lock actuator, Tailgate lock actuator
29 | 20 A | GRN/WHT | Driver's power window motor (via power window master switch)