## Water Pump Replacement

1. | Remove the drive belt.

2. | Drain the engine coolant.

3. | Remove the water pump pulley.

4. | Remove the five bolts securing the water pump, then remove the water pump (A).

5. | Inspect and clean the O-ring groove and mating surface with the cylinder block.

6. | Install the water pump with new O-ring (B) in the reverse order of removal.

7. | Clean up any spilled engine coolant.

8. | Refill the radiator with engine coolant, and bleed air from the cooling system with the heater valve open.