## A/T Park Pin Switch Test/Replacement

1. | Remove the center console.

2. | Disconnect the park pin switch connector (2P).

3. | Shift the shift lever into the [P] position, then check for continuity between the No. 1 and No. 2 terminals. There should be continuity.

4. | Shift the shift lever out of the [P] position, and check for continuity between the terminals in 3. There should be no continuity.

5. | If the park pin switch is faulty, remove the shift lever assembly, and replace the detent bracket. (The park pin switch is not available separately.)