## Center Console Removal/Installation

NOTE:

- When prying with a flat-tip screwdriver, wrap it with protective tape to prevent damage.
- Take care not to scratch the front seat, dashboard, and related parts.

1. | Remove the parking brake cover lid (A).

2. | M/T: Remove the shift knob.

3. | Remove the center console (A):
-1 | Remove the screws (B), and clips (C).
-2 | Lift the rear of the console up to detach the clip (D), and pull the console rearward to release the front hook (E) from the heater unit.
-3 | Disconnect the cigarette lighter connector (F).

4. | Install the console in the reverse order of removal, and note these items: Replace any damaged clips. Make sure the wire harness is not pinched. Set the rib (G) under the pocket onto the parking brake lever bracket (H) correctly.