## Valves, Springs and Valve Seals Installation

Special Tools Required
Stem seal driver ( 07PAD-0010000)

Valve spring compressor ( 07757-0010000)

1. | Coat the valve stems with engine oil. Install the valves in the valve guides.

2. | Check that the valves move up and down smoothly.

3. | Install the spring seats on the cylinder head.

4. | Install the new valve seals (A) using the valve guide seal installer (B). NOTE: The exhaust valve seal (C) has a black spring (D), and the intake valve seal (E) has a white spring (F). They are not interchangeable.

5. | Install the valve spring. Place the end of the valve spring with closely wound coils toward the cylinder head.

6. | Install the valve retainer.

7. | Install the valve spring compressor. Compress the spring, and install the valve keepers.

8. | Lightly tap the end of each valve stem two or three times with a plastic mallet (A) to ensure proper seating of the valve and valve keepers. Tap the valve stem only along its axis so you do not bend the stem.