## Rear Fender Cover Replacement

## For Some Models

NOTE: Take care not to scratch the rear fender cover and body.

1. | Remove the rear damper unit, refer to the 2002 Jazz/Fit Shop Manual, P/N 62SAA00.

2. | Remove the rear fender cover (A).
-1 | Remove the screws (B) securing the rear bumper (C) and rear fender cover.
-2 | Remove the bolts (D), and clips (E, F), then remove the rear fender cover.

3. | Install the rear fender cover in the reverse order of removal, and replace any damaged clips.