## OPDS Unit Replacement

NOTE: Review the seats replacement procedure in the body section before performing repair or service.

## Removal

1. | Disconnect the negative battery cable, and wait at least 3 minutes before beginning work.

2. | Disconnect the side airbag harness 2P connector.

3. | Remove the seat assembly and seat-back cover.

4. | Remove the cover (A), then disconnect the OPDS unit harness 8P and sensor connectors from the OPDS unit.

5. | Remove the two screws (B) and OPDS unit (C).

## Installation

1. | Place the new OPDS unit on the seat-back frame. Tighten the two screws (A), and connect the OPDS unit harness 8P and sensor connector to the OPDS unit. Reinstall the cover.

2. | Install the seat-back cover.

3. | Install the seat assembly, then connect the side airbag harness 2P connector.

4. | Reconnect the battery negative cable.

5. | Set the seat-back in the normal position, and make sure there is nothing sitting on the front passenger's seat.

6. | Initialize the OPDS unit.

7. | After installing the OPDS unit, confirm proper system operation: Turn the ignition switch ON (II); the SRS indicator should come on for about 6 seconds and then go off.