## Starter Solenoid Test

1. | Check the hold-in coil for continuity between the S terminal (A) and the armature housing (ground). There should be continuity. If there is continuity, go to 2. If there is no continuity, replace the solenoid.

2. | Check the pull-in coil for continuity between the S terminal (A) and M terminal (B). There should be continuity. If there is continuity, the solenoid is OK. If there is no continuity, replace the solenoid.