## Yaw Rate/Lateral Acceleration Sensor Replacement

NOTE:

- Do not damage or drop the sensor as it is sensitive.
- Do not use an impact wrench.

1. | Remove the center console.

2. | Pull down the carpet.

3. | Disconnect the yaw rate/lateral acceleration sensor 4P connector (A).

4. | Remove the sensor mounting bolts, and remove the yaw rate/lateral acceleration sensor (B).

5. | Install in the reverse order of removal.