## Power Mirror Actuator Test

1. | Remove the door panel.

2. | Disconnect the connector (A) from the power mirror actuator.

3. | Check actuator operation by connecting power and ground according to the table. 10P CONNECTOR: 6P CONNECTOR: 3P CONNECTOR:

4. | If the mirror fails to work properly, replace the mirror actuator.

### Defogger Test

5. | Check for continuity between the No. 4 and No. 10 terminals of the 10P connector, or between the No. 1 and No. 2 terminals of the 6P connector. There should be continuity.

### Retract Test

6. | Check actuator operation by connecting battery power and ground according to the table. 10P CONNECTOR: 6P CONNECTOR:

7. | If the retract actuator fails to work properly, replace the mirror.