## ATF Feed Pipe Replacement - End Cover

1. | Remove feed pipe flange plate (A), then remove the feed pipe (B) and feed pipe flange (C) from the end cover (D). NOTE: Replace the end cover, if the undetachable ATF feed pipes (E) replacement is required.

2. | Install the new O-ring (F) over the ATF feed pipe.

3. | Install the new O-ring (G) on the feed pipe flange.

4. | Install the feed pipe (A) through the feed pipe flange (B) with aligning the feed pipe tab (C) with the guide (D) on the flange. NOTE: The illustration shows the tabs and guides for sake of clarity.

5. | Install the ATF feed pipe over the undetachable feed pipe (E), and align the tab (F) of the feed pipe flange with the guide (G) on the end cover.

6. | Install the feed pipe flange plate.