## Instrument Visor Removal/Installation

NOTE:

- Do not pry the visor or panel surface with a flat-tip screwdriver to prevent damage.
- Take care not to scratch the dashboard and related parts.
- LHD is shown, RHD is symmetrical.

1. | Tilt the steering column down.

2. | Remove the instrument panel (A):
-1 | Gently pull out along the bottom to release the hooks (B), and ribs (C) from the clips (D) of the instrument lower visor (E).
-2 | Gently pull out the upper portion of the panel to detach the hooks (F) and clips (G, H).

3. | Remove the instrument lower visor (A):
-1 | Remove the screws (B).
-2 | Gently pull out along the top to release the clips (C).

4. | Remove the screws, then remove the instrument upper visor (A).

5. | Install the visors and panel in the reverse order of removal. Push the clip portions into place securely.