## Fuel Tank Replacement

1. | Drain the fuel tank: Remove the fuel pump. Using a hand pump, hose and container suitable for gasoline, draw the fuel from the fuel tank.

2. | Jack up the vehicle, and support it with jackstands.

3. | Disconnect the hoses (A). Slide back the clamps, then twist the hoses as you pull to avoid damaging them.

4. | Remove the fuel tank guard (B) and the center front floor cross beam (C).

5. | Place a jack, or other support, under the tank.

6. | Remove the strap bolts, and let the straps (D) fall free.

7. | Remove the fuel tank (E). If it sticks to the undercoat on its mount, carefully pry it off the mount.

8. | Install the remaining parts in the reverse order of removal.