## Blower Unit Removal and Installation

NOTE: LHD type is shown, RHD type is symmetrical.

1. | Remove the passenger's dashboard under cover and the inner glove box.

2. | Disconnect the recirculation control cable from the recirculation control linkage.

3. | Disconnect the connector (A) from the blower motor, then remove the mounting bolt, the self-tapping screws, and the bracket (B).

4. | Remove the clip (A). Remove the mounting bolt, the screws, and the bracket (B). Remove the connector clip (C). Remove the self-tapping screws and the blower unit (D).

5. | Install the unit in the reverse order of removal. Make sure that there is no air leakage.