## Radiator and Fan Replacement

1. | Drain the engine coolant.

2. | Remove the front bumper, and front bumper bracket.

3. | Remove the air cleaner housing.

4. | Remove the upper radiator hose, lower radiator hose and Automatic Transmission Fluid (ATF) cooler hoses.

5. | Disconnect the fan motor connector, and remove the upper bracket and cushion, then pull up the radiator.

6. | Remove the fan shroud assembly and other parts from the radiator.

7. | Install the radiator in the reverse order of removal. Make sure the upper and lower cushions are set securely.

8. | Install the air cleaner housing.

9. | Install the front bumper bracket, and apply body paint to the mounting bolts, then install the front bumper.

10. | Fill the radiator with engine coolant and bleed the air.