Steering
Item | Measurement | Qualification | Standard or New
--- | --- | --- | ---
Steering wheel | Rotational play measured at outside edge with engine running |  | 0-10 mm (0-0.39 in.)
Starting load measured at outside edge with engine running |  | 29 N (3.0 kgf, 6.6 Ibf)
Gearbox | Angle of rack guide screw loosened from locked position |  | 5 °±2 °

Suspension
Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Wheel alignment | Camber | Front | 0 ° 00 '±1 °
Rear | -1 ° 00 '± 1'
Caster | Front | 2 ° 10 '±1 °
Total Toe-in | Front | 0±3 mm (0±0.12 in.)
Rear | 2+2-1 mm (0.08+0.08-0.04 in.)
Front wheel turning angle equipped with 175/65R14 82T tyres | Inside wheel | 41 ° 00 '±2 °
Outside wheel | 36 ° 00 ' (Reference)
Front wheel turning angle equipped with 185/55R15 82V tyres | Inside wheel | 38 ° 00 '±2 °
Outside wheel | 34 ° 00 ' (Reference)
Wheel | Steel wheel runout | Axial | 0-1.0 mm (0-0.04 in.) | 2.0 mm (0.08 in.)
Radial | 0-1.0 mm (0-0.04 in.) | 1.5 mm (0.06 in.)
Aluminum wheel runout | Axial | 0-0.7 mm (0-0.03 in.) | 2.0 mm (0.08 in.)
Radial | 0-0.7 mm (0-0.03 in.) | 1.5 mm (0.06 in.)
Wheel bearing | End play | Front | 0-0.05 mm (0-0.002 in.)
Rear | 0-0.05 mm (0-0.002 in.)

Brakes
Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Parking brake lever | Distance travelled when lever pulled with 196 N (20 kgf, 44 Ibf) of force |  | 6 to 10 clicks
Brake pedal | Pedal height (carpet removed) | M/T | 141 mm (5.55 in.)
CVT | 145 mm (5.71 in.)
Free play |  | 1-5 mm (0.04-0.2 in.)
Master cylinder | Piston-to-pushrod clearance |  | 0-0.4 mm (0-0.02 in.)
Brake disc | Disc thickness | Front | 21.0 mm (0.83 in.) | 19.0 mm (0.75 in.)
Rear | 8.9-9.1 mm (0.35-0.36 in.) | 8.0 mm (0.31 in.)
Disc runout | Front and Rear | ——— | 0.10 mm (0.004 in.)
Disc parallelism | Front and Rear | ——— | 0.015 mm (0.0006 in.)
Pad thickness | Front | 9.0 mm (0.35 in.) | 1.6 mm (0.06 in.)
Rear | 6.8-7.5 mm (0.27-0.30 in.) | 1.6 mm (0.06 in.)
Brake drum | I.D. |  | 180 mm (7.09 in.) | 181 mm (7.13 in.)
Lining thickness |  | 4.3 mm (0.17 in.) | 1.0 mm (0.039 in.)
Brake booster - Rear brake disc | Master cylinder fluid pressure at 0 kPa (0 mmHg, 0 in.Hg) of vacuum with pressing brake pedal | Pressed with 98 N (10 kgf, 22 Ibf) | 0 kPa (0 kgf/cm2, 0 psi)
Pressed with 294 N (30 kgf, 66 Ibf) | 1,370 kPa (14.0 kgf/cm2, 199 psi)
Master cylinder fluid pressure at 66.7 kPa (500 mmHg, 19.7 in.Hg) of vacuum with pressing brake pedal | Pressed with 98 N (10 kgf, 22 Ibf) | 3,240 kPa (33.0 kgf/cm2, 470 psi)
Pressed with 294 N (30 kgf, 66 Ibf) | 8,240 kPa (84.0 kgf/cm2, 1,195 psi)
Brake booster - Rear brake drum (equipped with ABS) | Master cylinder fluid pressure at 0 kPa (0 mmHg, 0 in.Hg) of vacuum with pressing brake pedal | Pressed with 98 N (10 kgf, 22 Ibf) | 0 kPa (0 kgf/cm2, 0 psi)
Pressed with 294 N (30 kgf, 66 Ibf) | 1,550 kPa (15.8 kgf/cm2, 225 psi)
Master cylinder fluid pressure at 66.7 kPa (500 mmHg, 19.7 in.Hg) of vacuum with pressing brake pedal | Pressed with 98 N (10 kgf, 22 Ibf) | 4,110 kPa (41.9 kgf/cm2, 596 psi)
Pressed with 294 N (30 kgf, 66 Ibf) | 9,590 kPa (97.8 kgf/cm2, 1,391 psi)
Brake booster - Rear brake drum (without ABS) | Master cylinder fluid pressure at 0 kPa (0 mmHg, 0 in.Hg) of vacuum with pressing brake pedal | Pressed with 98 N (10 kgf, 22 lbf) | 0 kPa (0 kgf/cm2, 0 psi)
Pressed with 294 N (30 kgf, 66 lbf) | 1,600 kPa (16.3 kgf/cm2, 230 psi)
Master cylinder fluid pressure at 66.7 kPa (500 mmHg, 19.7 in.Hg) of vacuum with pressing brake pedal | Pressed with 98 N (10 kgf, 22 lbf) | 3,700 kPa (37.7 kgf/cm2, 537 psi)
Pressed with 294 N (30 kgf, 66 lbf) | 9,800 kPa (99.9 kgf/cm2, 1,421 psi)

Air Conditioning
Item | Measurement | Qualification | Standard or New
--- | --- | --- | ---
Refrigerant | Type |  | HFC-134a (R-134a)
Capacity of system |  | 400-450 g (14.1-15.9 oz)
Refrigerant oil | Type |  | KEIHIN SP-10 (P/N 38897-P13-003, 38898-P13-003 or 38899-P13-A01)
Capacity of components | Condenser | 25 mL (5/6 fl oz, 0.9 Imp oz)
Evaporator | 35 mL (1 1/6 fl oz, 1.2 Imp oz)
Each line and hose | 10 mL (1/3 fl oz, 0.4 Imp oz)
Compressor | 85-105 mL (2 5/6-3 1/2 fl oz, 3.0-3.7 Imp oz)
Compressor | Starter coil resistance | At 20 °C (68 °F) | 3.05-3.35 W
Pulley-to-pressure plate clearance |  | 0.35-0.65 mm (0.014-0.026 in.)